|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
|  | Your company name  Workplace Safety Assessment  Job Hazard Analysis (JHA) | | | | Your logo here |
| Document Control #: | Stone-JHA-006 | | | Revision Date: | mm/dd/yyyy |
| Document Title: | Job Hazard Analysis (JHA) | | | Issue #: | 1.0 |
| Department: | Warehousing | | | Frequency: | Annually |
| Personal Protective Equipment Required: | Safety glasses, gloves, safety vest, hearing protection | | | Completed by: | Name of Company Representative Here |
| Using a Reciprocating Saw | | | | | |
| Task Description | | Hazard | Control | | |
| Binding Blade | | Blade Breakage | * This is an indication that a bundle it trying to lean as pressure is released. Stop work and evaluate where pressure is coming from, ensure material is properly secured. Wear safety glasses | | |
| Excessive Wood Vibration | | Stuck By / Caught Between | * This is an indication that wood is loose somewhere (normally on the vertical supports). Stop work evaluate where boards may not adequately be secured/braced. Wear Safety glasses | | |
| Loss of Control | | Operator Injury / Product Damage | * Maintain a two hand grip and apply controlled pressure | | |
| Cutting Wood | | Noise | * Recommendation: Wear hearing protection (ear muffs or plugs) | | |

Rationale or Comment:

* + Use a blade designed for cutting wood with nails.

End of Document

**Disclaimer**

*This document is written as a general guideline. Natural Stone Institute and its Member companies have neither liability nor can they be responsible to any person or entity for any misunderstanding, misuses, or misapplication that would cause loss or damage of any kind, including loss of rights, material, or personal injury, or alleged to be caused directly or indirectly by the information contained in this document.*