|  |  |  |
| --- | --- | --- |
|  | Your company nameWorkplace Safety AssessmentJob Hazard Analysis (JHA)  | Your logo here |
| Document Control #: | Stone-JHA-018 | Revision Date: | mm/dd/yyyy |
| Document Title: | Job Hazard Analysis (JHA)  | Issue #: |  |
| Department: | (name) | Frequency: | (Annually, monthly, weekly) |
| Personal Protective Equipment Required: | Safety glasses, gloves, safety vest | Completed by: | Name of Company Representative Here |
| Applying Thinset to Substrate |
| Task Description | Hazard | Control |
| Applying Thinset to Substrate | Eye InjurySkin Irritation  | * Keep exposed skin clean at all times when using portland products
* Immediately wash thinset or grout off skin
 |

End of Document

**Disclaimer**

*This document is written as a general guideline. Natural Stone Institute and its Member companies have neither liability nor can they be responsible to any person or entity for any misunderstanding, misuses, or misapplication that would cause loss or damage of any kind, including loss of rights, material, or personal injury, or alleged to be caused directly or indirectly by the information contained in this document.*