|  |  |  |
| --- | --- | --- |
|  | Your company nameWorkplace Safety AssessmentJob Hazard Analysis (JHA)  | Your logo here |
| Document Control #: | Stone-JHA-021 | Revision Date: | mm/dd/yyyy |
| Document Title: | Job Hazard Analysis (JHA)  | Issue #: |  |
| Department: | (name) | Frequency: | (Annually, monthly, weekly) |
| Personal Protective Equipment Required: | Safety glasses, gloves, safety vest | Completed by: | Name of Company Representative Here |
| Cutting Tile with Tile Break |
| Task Description | Hazard | Control |
| Cutting tile with tile break (snap or rail cutter) | Cuts to hands, fingersEye Injury | * Ensure cutting wheel is sharp
* Check cut edge for sharp surface irregularities
 |

Rationale or Comment:

* Cuts are never as clean as cuts made with a wet tile saw.
* Place cut edge against wall were it will be covered with baseboard.

End of Document

**Disclaimer**

*This document is written as a general guideline. Natural Stone Institute and its Member companies have neither liability nor can they be responsible to any person or entity for any misunderstanding, misuses, or misapplication that would cause loss or damage of any kind, including loss of rights, material, or personal injury, or alleged to be caused directly or indirectly by the information contained in this document.*