|  |  |  |
| --- | --- | --- |
|  | Your company nameWorkplace Safety AssessmentJob Hazard Analysis (JHA)  | Your logo here |
| Document Control #: | Stone-JHA-022 | Revision Date: | mm/dd/yyyy |
| Document Title: | Job Hazard Analysis (JHA)  | Issue #: |  |
| Department: | (name) | Frequency: | (Annually, monthly, weekly) |
| Personal Protective Equipment Required: | Safety glasses, hearing protection, dust mask, gloves, safety vest | Completed by: | Name of Company Representative Here |
| Cutting Tile with 4” Grinder |
| Task Description | Hazard | Control |
| Operating 4” grinder | Electrocution | * Connect grinder to a Ground Fault Circuit Interrupter (GFCI) outlet
* Do not use extension cords without a grounding wire
 |
| Cutting tile | Noise  | * Properly wear hearing protection (ear muffs or plugs)
 |
| Cuts to hands, fingersEye InjuryDust inhalation | * Ensure blade is installed correctly
* Ensure all guards are in place
* Check cut edge for sharp surface irregularities
* Wear dust mask if dry cutting
 |

Rationale or Comment:

* Keep all cords clear of cutting area.
* Remove jewelry.
* Do not wear baggy clothing.

End of Document

**Disclaimer**

*This document is written as a general guideline. Natural Stone Institute and its Member companies have neither liability nor can they be responsible to any person or entity for any misunderstanding, misuses, or misapplication that would cause loss or damage of any kind, including loss of rights, material, or personal injury, or alleged to be caused directly or indirectly by the information contained in this document.*