|  |  |  |
| --- | --- | --- |
|  | Your company nameWorkplace Safety AssessmentJob Hazard Analysis (JHA)  | Your logo here |
| Document Control #: | Stone-JHA-015 | Revision Date: | mm/dd/yyyy |
| Document Title: | Job Hazard Analysis (JHA)  | Issue #: |  |
| Department: | (name) | Frequency: | (Annually, monthly, weekly) |
| Personal Protective Equipment Required: | Hardhat, Safety glasses, Safety vest  | Completed by: | Name of Company Representative Here |
| Unloading or Moving Material |
| Task Description | Hazard | Control |
| Unloading or moving material | Back injuries, pinched or smashed extremities  | * Lift properly using legs
* Keep back straight
* Use pallet jack
* Confirm lay-down area is free of debris and holes
 |
| Head injuries |
| Trips and falls |

Rationale or Comment:

* + Always complete a pre-movement inspection.

End of Document

**Disclaimer**

*This document is written as a general guideline. Natural Stone Institute and its Member companies have neither liability nor can they be responsible to any person or entity for any misunderstanding, misuses, or misapplication that would cause loss or damage of any kind, including loss of rights, material, or personal injury, or alleged to be caused directly or indirectly by the information contained in this document.*